{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Environmental conditions"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Environmental conditions","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[[21,0,21,1],[20,0,20,1],[2,1,2,2],[2,3,2,4],[2,0,3,0]]}
["Table C.1 - Internal and external conditions used for analysis"]
[]
["Month","Internal",null,"External"]
[null,"deg.C","0-1","deg.C","0-1"]
["Oct",20,0.56999999999999995,10,0.83]
["Nov",20,0.56999999999999995,5,0.88]
["Dec",20,0.59,1,0.88]
["Jan",20,0.56999999999999995,-1,0.85]
["Feb",20,0.57999999999999996,0,0.84]
["Mar",20,0.54,4,0.78]
["Apr",20,0.51,9,0.72]
["May",20,0.51,14,0.68]
["Jun",20,0.5,18,0.69]
["Jul",20,0.56000000000000005,19,0.73]
["Aug",20,0.52,19,0.75]
["Sep",20,0.56000000000000005,15,0.79]
[]
[]
["Surface Resistance (m2K/W)"]
[]
["External resistance",null,0.04]
["Internal resistance",null,0.13]
[]
[]
["Interstitial Condensation Analysis"]